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200 rue Bank

Sherbrooke, QC J1H 4K3
Division 09 - Finishing

Section 096513.23 – Resilient Stair Treads and Risers
ABDEFENDER® Stair Treads
This document is intended as a suggested guide for editing your architectural guide specification. 

American Biltrite will not be held liable for damages arising out of the use of any information or specifications found in this document. Make sure you have the latest publication for this specification. 

Product selection and accuracy of all project specifications are the specifier’s or designer’s responsibility.

PART 1 – GENERAL INFORMATION

1.01 summary
A. This section deals with resilient flooring found in the drawings and schedules of the contract that meet the requirements of this section. 

1.02
RELATED SECTIONS 

A. Section 3 – Cement: not covered in this section.

B. Section 6 – Wood and plastic: not covered in this section.

C. Section 7 – Thermal and humidity protection: not covered in this section.

D. Section 9 – Other sections containing information related to floor finishes: not covered in this section.
1.03
rEfErences (INDUSTRY standards)

A. ASTM F710: « Practice for preparing concrete floors to receive resilient flooring ». 

B. ASTM E648: « Test method for critical radiant flux of floor covering systems using a radiant heat energy source ». 

C. ASTM E662: « Test method for specific optical density of smoke generated by solid materials ». 

D. ASTM F2169: « Standard specification for Resilient Stair Treads ».
E. ASTM F970: « Standard test method for measuring static load limit ».
F. ASTM E84: « Surface burning characteristics of building materials ».

G. CAN/ULC S102.2: « Surface burning characteristics of building materials ».
1.04
items TO DELIVER

A. Provide the product’s Technical Specifications data sheet as well as all Installation and Maintenance Instructions.

B. When required, supply floor drawings and installation plans.

C. Supply a set of samples measuring at least 12 cm (5 in) by 12 cm (5 in) of the complete range of colors and finishes chosen for the project.

D. When required, provide American Biltrite’s attestation, certified by an independent laboratory, confirming that the flooring complies with the fire standards of the following tests:

1.
ASTM E648; Critical Radiant Flux: 0.45 watts/cm2 or more;

2.
ASTM E662; Smoke Density: 450 or less;

3.
ASTM E84; Class A; 

4.
CAN/ULC S102.2; FSV ≤ 25 and SDV ≤ 50.

E. Provide American Biltrite’s Warranty Certificate.
1.05
QUALITY ASSURANCE

A. Have American Biltrite flooring installed by a qualified installer of this type of flooring.

B. In accordance with the technical instructions in the Installation Instructions, use all the accessories recommended by American Biltrite when installing its flooring.
C. Follow the instructions specified in the most recent version of American Biltrite’s Installation Instructions.

D. Manufactured in a factory that has ISO 9001 and ISO 14001 certifications.

1.06
DELIVERY, HANDLING, STORAGE

A. Deliver the flooring to the installation site in American Biltrite’s original packaging. Indicate the project name and handling instructions on the outside of the boxes.

B. Advise the carrier of any damaged material and indicate it on the packing slip.

C. Store the flooring inside, sheltered from extreme hot or cold temperatures. Place the material on a smooth level floor or where there is uniform solid support in a clean, dry well-ventilated area. Unstack the palettes. The long-term storage temperature must be maintained between 18°C (65°F) and 29°C (85°F). Protect adhesive and flooring material from freezing, extreme heat, and direct sun exposure.

D. Acclimatize the subfloor, all flooring material and adhesives for 48 hours before, during and 72 hours after the installation by maintaining the room temperature between 18°C (65°F) and 29°C (85°F). The palettes should be unstacked 24 hours prior to use.

E. Afterwards, maintain the room temperature between 13°C (55°F) and 38°C (100°F). Protect the material from direct sources of heat such as air vents and other types of heaters.

F. Install the flooring after all other finishing work, including painting, has been completed.
PART 2 - PRODUCTS

2.01 Manufacturer

A. American Biltrite 
200 Bank Street
Sherbrooke, QC, Canada, J1H 4K3
Telephone: 819-829-3300

Toll free: 1-800-437-8743
Internet: www.american-biltrite.com
2.02 resilient flooring description AND MINIMUM PERFORMANCE CRITERIA 
A. Characteristics: 

1. ABDEFENDER® Stair Tread complies with Resilient Stair Tread ASTM F2169, Type TS, Class 2. Group 1 also available. 
2. Nominal thickness: 3.17 mm (1/8 in.) 

3. Sizes:

a) Stair Treads: width: 314 mm (12 3/8 in.); length: 914 mm (36 in.) or 1,219 mm (48 in.) or 1,828 mm (72 in.).

b) Stair Tread + Riser: width: 482 mm (19 in.); length: 914 mm (36 in.) or 1,219 mm (48 in.) or 1,828 mm (72 in.)
4. Meets ASTM E84, Class A.
5. Meets CAN/ULC S102.2, FSV ≤ 25 and SDV ≤ 50.
6. Meets ASTM F970 static load limit.
7. Needs to be FloorScore® certified.

8. Needs to be certified Declare Red List Free. 

9. Needs to have a third party certified environmental product declaration EPD type III.
10. Refer to the product’s Technical Specifications data sheet for detailed specifications.

11. Choose from any of American Biltrite’s complete line of colors (indicate the item number).

2.03 AdhEsives

A. Use American Biltrite’s Zip Step tape. The tape covers 50 m (164 lin. feet). Also, AD-777 or AD-590 adhesive can be used. AD-777 and AD-590 both cover 18.6 sq. m/3.8 liters (200 sq. ft./gallon) when applied with the recommended notched trowel.
B. NC-888 compound must be used on all tread’s nosing.
2.04 other material

A. Subfloor repairs: use a good-quality Portland cement-based compound that has a minimal resistance to compression of 246 kg/cm2 (3,500 lb./sq. in) to fill, smooth or level subfloor imperfections.

B. Self-levelling underlayment: use a Portland cement-based self-levelling underlayment that has a minimal resistance to compression of 246 kg/cm2 (3,500 lb./sq. in).

PART 3 – EXECUTION

3.01 
SITE INSPECTION
A. Examine the subfloor before installation to ensure that the surface is clean, dry, smooth, structurally sound, and free from foreign substances that may adversely affect adhesion or cause discoloration. Furthermore, ensure that the subfloor is free of paint, varnish, adhesive, oil, grease, solvent, and other foreign substances, including treatment compounds, sealers and curing compounds that may adversely affect adhesion or alter the appearance or durability of the rubber flooring.

B. Verify the surface to ensure there is no powder, scaling or mold. If there is, remove it with a mechanical sander and level with a good-quality cement-based Portland primer.
C. If the following situations occur on site, refer to the “Remediation System” document:

· Sealers, curing agents or hardeners were used in/on the concrete.

· Chemical abatement was used to remove the old flooring.
D. Report and rectify all unsatisfactory conditions. Do not start flooring installation until all rectifications have been completed.

3.02 
SUBFLOOR PREPARATION

A. Level all rough surfaces and fill cracks and marks with a Portland cement-based patching compound.

B. Mechanically remove all surface contaminants such as paint, oil, grease, varnish, adhesive as well as various other products such as treatment compounds. Do not use solvent-based stripper.
C. In case of doubt, test the adhesion on the cement subfloor or other surface that will be covered by the flooring. Do the test using the specified flooring and recommended adhesive.

3.03 
RESILIENT FLOORING INSTALLATION

A. Install the flooring according to the latest version of American Biltrite’s Installation Instructions. Use the tools, adhesives, trowel types and procedures recommended in the instructions.

B. Acclimatize the subfloor, all flooring material and adhesives for 48 hours before, during and 72 hours after the installation by maintaining the room temperature between 18°C (65°F) and 29°C (85°F). Afterwards, maintain the temperature between 13°C (55°F) and 38°C (100°F).

3.04 
CLEANING AND PROTECTION

A. Remove all excess adhesive immediately after installation as recommended in American Biltrite’s Installation Instructions.

B. Before allowing traffic after installation, consult and follow the recommendations in American Biltrite’s Installation Instructions.

C. Following installation and cleanup, if the work of all other trades has not yet been completed, protect the flooring by laying sheets of non-staining brown Kraft paper, and then a layer of plywood sheets (rolls of non-staining heavy cardboard material could also be used for protection). 

D. Follow the instructions in American Biltrite’s Maintenance Instructions when performing initial and regular maintenance procedures.

END OF SECTION 096513.23
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Please note that technical web site documents prevail. 
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